

Make the Img file


Folder Direction



CMD window



Change it to .img to bin



Copy to bin file

C:\ti\mcsdk\_2\_01\_01\_04\tools\writer\nor\evmc6657l\bin

nor\_writer\_input.txt


file\_name = app.bin

start\_addr = 2097152

Run->Load


C:\ti\mcsdk\_2\_01\_01\_04\tools\writer\nor\evmc6657l\bin-> norwriter\_evm6657l.out file

View->Memory Browser->


ㅋStart address: 0x80000000

Mouse right ->Load Memory


C:\ti\mcsdk\_2\_01\_01\_04\tools\writer\nor\evmc6657l\bin




Next




Finish





Run

You see below on the Console



You can show after nor programming completed successfully.